<PropertyList>

    <name>Pushback and Start</name>
    <description>
We're now fully configured to begin our pushback and engine start. The passengers are on board and you've just been given your clearance. As things start to happen very quickly from here on out, don't be afraid to pause your sim between steps.
    </description>
    <audio-dir>Aircraft/747-400/tutorial</audio-dir>
    <timeofday>noon</timeofday>

    <init>
      <set>
        <property>/controls/gear/brake-parking</property>
        <value>1</value>
      </set>
      <set>
        <property>/controls/flight/flaps</property>
        <value>0.0</value>
      </set>
      <set>
        <property>/controls/engines/engine/magnetos</property>
        <value>0</value>
      </set>
      <set>
        <property>/controls/engines/engine/throttle</property>
        <value>0</value>
      </set>
      <set>
        <property>/engines/engine/running</property>
        <value>false</value>
      </set>
      <set>
        <property>/instrumentation/adf/frequencies/selected-khz</property>
        <value>340</value>
      </set>
      <set>
        <property>/environment/weather-scenario</property>
        <value>Fair weather</value>
      </set>
      <set>
        <property>/controls/flight/elevator-trim</property>
        <value>0.17</value>
      </set>
    </init>

    <step>
      <message>Close all doors.</message>
    </step>

    <step>
      <message>Turn ON the BEACON lights.</message>
	<view>
		<heading-offset-deg>319.9</heading-offset-deg>
		<pitch-offset-deg>26.2</pitch-offset-deg>
		<roll-offset-deg>0.0</roll-offset-deg>
		<x-offset-m>-0.55</x-offset-m>
		<y-offset-m>3.8</y-offset-m>
		<z-offset-m>-23.5</z-offset-m>
		<field-of-view>57</field-of-view>
	</view>
	<exit>
	<condition>
		<equals>
			<property>/controls/lighting/beacon</property>
			<value>1</value>
		</equals>
	</condition>
	</exit>
    </step>

    <step>
      <message>Set Hydraulid DEMAND Pump selector 4 to AUX.</message>
    </step>

    <step>
      <message>Set Hydraulic DEMAND Pump selectors 1-3 to AUTO.</message>
    </step>

    <step>
      <message>Turn OFF all but one PACK selector.</message>
    </step>

    <step>
      <message>Turn OFF autostart.</message>
    </step>

    <step>
      <message>Turn ON continuous ignition.</message>
      <marker>
		<x-m> 0.0198</x-m>
		<y-m>-0.0835</y-m>
		<z-m>-0.0033</z-m>
		<scale>1.6777</scale>
	</marker>
	<exit>
	<condition>
		<equals>
			<property>/controls/engines/con-ignition</property>
			<value>1</value>
		</equals>
	</condition>
	</exit>
    </step>

    <step>
      <message>Ensure all throttles are at idle</message>
	<exit>
	<condition>
		<equals>
			<property>/controls/engines/engine[0]/throttle</property>
			<value>0</value>
		</equals>
		<equals>
			<property>/controls/engines/engine[1]/throttle</property>
			<value>0</value>
		</equals>
		<equals>
			<property>/controls/engines/engine[2]/throttle</property>
			<value>0</value>
		</equals>
		<equals>
			<property>/controls/engines/engine[3]/throttle</property>
			<value>0</value>
		</equals>
	</condition>
	</exit>
    </step>

    <step>
      <message>ARM the emergency lights.</message>
    </step>

    <step>
      <message>Press the ENG button on the EICAS MCP.</message>
      <marker>
		<x-m>0.4174</x-m>
		<y-m>0.2041</y-m>
		<z-m>0.2595</z-m>
		<scale>0.9174</scale>
	</marker>
	<exit>
	<condition>
		<equals>
			<property>/instrumentation/eicas/display</property>
			<value>ENG</value>
		</equals>
	</condition>
	</exit>
    </step>

    <step>
      <message>Pull the Engine Start Selector for Engine 4.</message>
      <marker>
		<x-m>-0.0207</x-m>
		<y-m>0.0116</y-m>
		<z-m>-0.0033</z-m>
		<scale>1.2810</scale>
	</marker>
	<exit>
	<condition>
		<equals>
			<property>/controls/engines/engine[3]/starter</property>
			<value>1</value>
		</equals>
	</condition>
	</exit>
    </step>

    <step>
      <message>When the N2% RPM indicator on the EICAS reaches the magenta line (around 14%), switch the Fuel Control Switch for Engine 4 to RUN.</message>
	<exit>
	<condition>
		<equals>
			<property>/controls/engines/engine[3]/cutoff</property>
			<value>0</value>
		</equals>
	</condition>
	</exit>
    </step>

    <step>
      <message>Repeat this process for engine 1. Pull the Start Selector, wait for N2 to reach the magenta line, set Fuel Control to RUN.</message>
	<exit>
	<condition>
		<equals>
			<property>/controls/engines/engine[0]/cutoff</property>
			<value>0</value>
		</equals>
	</condition>
	</exit>
    </step>

    <step>
      <message>Now do the same thing for engines 2 and 3.</message>
	<exit>
	<condition>
		<equals>
			<property>/controls/engines/engine[1]/cutoff</property>
			<value>0</value>
		</equals>
		<equals>
			<property>/controls/engines/engine[2]/cutoff</property>
			<value>0</value>
		</equals>
	</condition>
	</exit>
    </step>

    <step>
      <message>Turn OFF the APU.</message>
	<exit>
	<condition>
		<equals>
			<property>/controls/APU/off-start-run</property>
			<value>0</value>
		</equals>
	</condition>
	</exit>
    </step>

    <step>
      <message>Turn OFF APU Bleed Air.</message>
    </step>

    <step>
      <message>Turn all PACK selectors to NORM.</message>
     </step>

    <step>
      <message>Set Hydraulid DEMAND Pump selector 4 to AUTO.</message>
    </step>

    <step>
      <message>Check the main display for any warnings.</message>
    </step>

    <step>
      <message>Turn ON MAIN and OVRD fuel pumps for each tank that contains fuel.</message>
    </step>
</PropertyList>
